SUBARU96 ECU connection list
The layout of the connectors is viewed from the wire side looking in at the ECU. The
Largest plug has been named "D" Moving From left to right we then have "C","B","A".
-----~----- 	-----~----- 	-----~----- 	-----~-----
|D13|~|D01|	|C08|~|C01| 	|B06|~|B01| 	|A11|~|A01|
|D26|~|D14| 	|C16|~|C09| 	|B12|~|B07| 	|A22|~|A12|
-----~----- 	-----~----- 	-----~----- 	-----~-----
PIN 	NO. 	DESCRIPTION
A01 	132
A02 	131 	power 12v from main relay
A03 	52 	boost pressure sensor +5V (****Pin C of Map Sensor****)
A04 	51 	boost MAP pressure signal (****Pin B of Sensor****)
A05 	50 	*(intake air temp signal)******
A06 	49 	oxygen sensor signal
A07 	48 	Coolant water temp signal
A08 	47 	air flow sensor supply
A09 	46 	MAF air flow sensor signal
A10 	45 	air flow sensor 0V not used
A11 	121 	Earth control unit
B01 	38 	throttle sensor 0V
B02 	37 	throttle sensor sig
B03 	36 	throttle sensor 5V
B04 	35 	crank angle signal
B05 	34 	crank angle sensor 0V
B06 	33 	crank angle shield GND
C01 	24 	cam sensor signal
C02 	23 	cam sensor 0V
C03 	22 	cam sensor shield GND
C04 	21 	knock sensor screen
C05 	20 	knock signal
C06 	19 	idle switch not used
C07 	18 	serial comms RX
C08 	17 	serial comms TX
D01 	112 	idle speed control
D02 	111 	idle speed control
D03 	8	wastegate solenoid
D04 	7	Rad fan
D05 	6	eng diode main relay
D06 	5	purge ****(water injection /water spray relay)*****
D07 	4	igniter pin 1
D08 	3	igniter pin 2
D09 	2	igniter pin 3
D10 	1	igniter pin 4
D11 	103 	injector 3
D12 	102 	injector 2
D13 	101 	injector 1






-----~----- 	-----~----- 	-----~----- 	-----~-----
[bookmark: _GoBack]|D13|~|D01|	|C08|~|C01| 	|B06|~|B01| 	|A11|~|A01|
|D26|~|D14| 	|C16|~|C09| 	|B12|~|B07| 	|A22|~|A12|
-----~----- 	-----~----- 	-----~----- 	-----~-----
PIN 	NO. 	DESCRIPTION
A12 	134 	not used
A13 	133 	power 12v from main relay
A14 	60 	insulation check
A15 	59 	permanent power supply
A16 	58 	Barometric altitude sensor not used
A17 	57 	oxygen sensor screen 0V
A18 	56 	not used
A19 	55 	0v screen air meter
A20 	54 	detection of transmission not used
A21 	53 	sensors 0V barometric air (**** pin A of map sensor ****)
A22 	122 	earth
B07 	44 	not used
B08 	43 	atmos 2 sig
B09 	42 	parking switch Anti-Lag (PBW) switch active when grounded
B10 	41 	neutral switch not used
B11 	40 	speedo signal
B12 	39 	ign key switch
C09 	32 	*9 AC switch not used
C10 	31 	starter switch not used
C11 	30 	accel not used
C12 	29 	diagnosis read memory not used
C13 	28 	diagnosis test mode not used
C14 	27 	not used
C15 	26 	trouble code output not used
C16 	25 	engine speed output
D14 	114 	earth
D15 	113 	earth ignition
D16 	16 	Power steering swt
D17 	15 	Rad fan
D18 	14 	ti monitor not used
D19 	13 	malfunction light oil press warning not used
D20 	12 	press exchange solenoid
D21 	11 	********Wastegate invert******
D22 	10 	rad fan AC Relay
D23 	9	fuel pump relay
D24 	106 	inj earth
D25 	105 	inj earth
D26 	104	injector 4
